**Which type of paint do I need?**

The following is **suggested guidance only**. Please refer to manufacturer’s instructions on tin before applying paint.

|  |  |
| --- | --- |
| **Surface to be painted:** | **Suggested paint types:** |
| **INSIDE WALLS & CEILINGS** Lounge, Dining Rooms, Hallways, Bedrooms | **EMULSION MATT** or **EMULSION SILK** or **WATER-BASED EGGSHELL** or **WATER-BASED SATIN(WOOD)***Silk emulsion has a shinier finish than matt, so is easier to clean* |
| **INSIDE WALLS & CEILINGS**Kitchen, Bathroom, WC | **KITCHEN & BATHROOM PAINT** or **WATER-BASED EGGSHELL** or **WATER-BASED SATIN(WOOD)***K&B paint is moisture resistant and protects against condensation* |
| **INSIDE & OUTSIDE WOOD & METAL** Doors, Window Frames, Skirting Boards, Furniture | **GLOSS** *Gloss paint has a shiny finish***SATIN(WOOD)** *Satin(wood) has a softer finish than gloss***EGGSHELL** *Eggshell has a duller matt finish than gloss & satin(wood)**Wood and Metal paint can be for interior or exterior use, refer to tin* |
| **INSIDE & OUTSIDE WOOD ONLY** Doors, Window Frames, Skirting Boards, Furniture | **WOODSTAIN** *can be for interior or exterior use, refer to tin***VARNISH** *can be for interior or exterior use, refer to tin***TIMBERCARE** *for outside garden furniture and fences only* |
| **BARE WOOD & METAL (SURFACE PREPARTION)**Doors, Window Frames, Skirting Boards, Furniture | **UNDERCOAT** *can be for interior or exterior use, refer to tin***PRIMER** *for wood or metal, interior or exterior use, refer to tin* |
| **EXTERIOR BRICKWORK AND MASONRY**  | **MASONRY PAINT** |
| **OTHER SURFACES** | **FLOOR PAINT, TILE PAINT, PLASTER PRIMER**  |

**FRP The Paint Place,** [**www.frponline.org.uk**](http://www.frponline.org.uk)

****

**How much paint will I need?**

Dulux have an [online paint calculator](http://www.dulux.co.uk/calculator/). Visit <http://www.dulux.co.uk/calculator/> to help estimate the number of litres of paint you require for the surface and area to be painted.

The following table is **suggested guidance only**. Please refer to manufacturer’s instructions on tin before applying paint. Spreading rate and coverage will depend on how porous the surface to be painted is. More than one coat may be required.

|  |
| --- |
| **One litre of emulsion paint** for **inside walls/ceilings** will cover **13m2** (one coat) |
| 2.5 litre tin emulsion matt/silk | will cover approx. 32m2 |
| 5 litre tin emulsion matt/silk | will cover approx. 64m2 |
| 10 litre tin emulsion matt/silk | will cover approx. 128m2 |
| **One litre of gloss paint** for **wood/metal** will cover **12m2 to 16m2** (one coat) |
| 750ml tin gloss paint | will cover approx. 9m2 |
| 2.5 litre tin gloss paint | will cover approx. 30m2 |
| 5 litre tin gloss paint | will cover approx. 60m2 |
| **One litre of exterior masonry paint** for **exterior brickwork** will cover **15m2** (on coat) |
| 5 litre tin masonry paint | will cover approx. 75m2 |
| 10 litre tin masonry paint | will cover approx. 150m2 |

**FRP The Paint Place,** [**www.frponline.org.uk**](http://www.frponline.org.uk)